
DNS Server
1. Lakukan login sebagai root pada terminal
#su
2. Lakukan installasi paket tersebut dengan perintah
#apt-get install bind9

3. Setelah melakukan installasi terbentuk Konfigurasi file yang ada di /etc/bind dan baca file named.conf, named.conf.local dan named.conf.option

Berikut ini adalah isi file named.conf, tidak perlu merupakan perubahan terhadap file ini.
// This is the primary configuration file for the BIND DNS server named.

// Please read /usr/share/doc/bind9/README.Debian.gz for information on the 

// structure of BIND configuration files in Debian, *BEFORE* you customize 

// this configuration file.

// If you are just adding zones, please do that in /etc/bind/named.conf.local

include "/etc/bind/named.conf.options";

// prime the server with knowledge of the root servers

zone "." {


type hint;


file "/etc/bind/db.root";

};

// be authoritative for the localhost forward and reverse zones, and for

// broadcast zones as per RFC 1912

zone "localhost" {


type master;


file "/etc/bind/db.local";

};

zone "127.in-addr.arpa" {


type master;


file "/etc/bind/db.127";

};

zone "0.in-addr.arpa" {


type master;


file "/etc/bind/db.0";

};

zone "255.in-addr.arpa" {


type master;


file "/etc/bind/db.255";

};

include "/etc/bind/named.conf.local";

Selanjutnya terdapat file named.conf.local, awalnya isi file ini masih kosong, isi dengan zona domain yang akan kita buat serta reverse domain sbb :

//

// Do any local configuration here

// Consider adding the 1918 zones here, if they are not used in your

// organization

//include "/etc/bind/zones.rfc1918";

zone "takehome.com" { // zona domain

type master; //tipe domain

file "/var/cache/bind/db.takehome"; //berisi file domain kita 
};

zone "108.252.10.in-addr.arpa" { //zona reverse diisi dengan no_network_id yang dibalik penulisannnay

type master;


file "/var/cache/bind/db.reverse"; // berisi file reverse kita
};


file named.conf.option berisi option tambahan pada domain kita, isikan sbb :

options {


directory "/var/cache/bind";


// If there is a firewall between you and nameservers you want


// to talk to, you may need to fix the firewall to allow multiple


// ports to talk.  See http://www.kb.cert.org/vuls/id/800113


query-source address * port 53;


// If your ISP provided one or more IP addresses for stable 


// nameservers, you probably want to use them as forwarders.  


// Uncomment the following block, and insert the addresses replacing 


// the all-0's placeholder.


forwarders {


 
202.154.178.2;



202.154.178.3;


};


auth-nxdomain yes;    # conform to RFC1035


listen-on-v6 { any; };

};

Selanjutnya siapkan dua file sesuai isi file yang ada pada file named.conf.local yaitu /cache/bind/db.takehome dan /var/cache/bind/db.reverse. Pindah ke direktori /var/cache/bind dan buat 2 file : db.takehome.com dan db.reverse, sesuaikan contoh dibawah dengan konfigurasi no ip komputer anda dan nama domain yang anda buat.
File db.takehome :

;

; BIND data file for local loopback interface

;

$TTL
604800

@
IN
SOA
localhost. root.localhost. (




      2

; Serial




 604800

; Refresh




  86400

; Retry




2419200

; Expire




 604800 )
; Negative Cache TTL

;

@
IN
NS
localhost.

@
IN
A
10.252.108.198

www
IN
A
10.252.108.198

mail
IN
A
10.252.108.198

file
IN
A
10.252.108.198

proxy
IN
A
10.252.108.198

File db.reverse :

;

; BIND reverse data file for broadcast zone

;

$TTL
604800

@
IN
SOA
localhost. root.localhost. (




      1

; Serial




 604800

; Refresh




  86400

; Retry




2419200

; Expire




 604800 )
; Negative Cache TTL

;

@
IN
NS
localhost.

198
IN
PTR
www.takehome.com

198
IN
PTR
mail.takehome.com

198
IN
PTR
file.takehome.com

198
IN
PTR
proxy.takehome.com

Selanjutnya Edit file /etc/resolv.conf tambahkan kata di bawah pada bagian paling atas atau ubah sesuai dengan konfigurasi komputer anda

nameserver 10.252.108.198

Lakukan restart pada komputer anda

#/etc/init.d/bind9 restart

4. Lakukan testing hasil percobaan installasi dan konfigurasi paket yang sudah dilakukan denagn command berikut ini. Jika tidak ada error berarti berhasil.
#nslookup 
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Gambar 2. Hasil Percobaa
Virtual Domain

1. Edit file /etc/bind/named.conf.local, tambahkan configurasi virtual domain

[image: image2.png]root@ubuntu:

Do any local configuration here

Consider adding the 1918 zones here, if they are not used in your
organization

//include "/etc/bind/ zones.rfe1918";
zone "takehome.com” { // zona domain
type master; //tipe domain

file "/var/cache/bind/ds.akehone; //berisi file domain kita
)

zone "44.252.10.in-addr.arpa” { //zoma reverse diisi dengan no_network_id y
ang dibalik penulisannnay N N
type master;
file "/var/cache/bind/db.reverse”; // berisi file reverse kita

)
include "/var/cache/bind/virtualdonain.cont”;





2. Buat file virtualdomain.conf pada direktori yang sudah ditentukan isikan nama domain yang akan dibuat, misal  domain admin.info dan jarkom.info sbb :

[image: image3.png]root@ubuntu: /var/cache/bind
Bons "acwin.inze” ( // zona Gowain
type master; //tipe acmain
Tile 7/var/cace/ning/dn.adwin. into"; //berisi Tile domein kit
)

zone "jarkom. infor (
type master;
file "/var/cache/bind/db.jarkom. info";





3. Buat dua file domain tersebut copikan dari filedomain yang sudah ada misal db.takehome.com

4. Selanjutnya restart dns server
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rootBupuntu: /var/cache/bindf s
db.reverse db.takehome virtualdomain.conf

rootBubuntu: /var/cache/bind§ cp db.takehome db.adwin.info

rootBubuntu: /var/cache/bindf cp db.takehome db.jarkon.info

rootBupuntu: /var/cache/bind§ /etc/init.d/bindd restart

* Stopping domain name service... bindd [ oK ]





5. Lakukan testing dengan ping ke domain baru

[image: image5.png]root@ubuntu: fyar/cache/bind
rootBupuntu: /var/cache/bind# ping vwv.adoin.info
PING www.admin.info (10.252.44.75) 56(54) bytes of data.
from file.takehome.com (10.252.44.75): icmp_seq=i tt.

£rom www. takehome.com (10.252.44.75) 1 icmp_se

from proxy.takehome.com [10.252.44.75): icwp_seq3 ttl=64 time=0.0

from adwin. takehome.com [10.252.44.75): icwp_seq=4 ttl=64 time=0.0

-~ wwv.aamin.info ping stavistics
4 packets transmitted, 4 received, 0% packet loss, time 3000ms
ret min/avy/max/ndev = 0.030/0.037/0.042/0.004 s

root@ubuntu: /var/cache/bind# vim /etc/bind/named.conf. local







































