Edit /etc/bind/named.conf tambahkan baris berikut ini :

controls {

        inet 127.0.0.1 allow {localhost; } keys { "rndc-key"; };

};

Edit /etc/bind/named.conf.local tambahkan beberaa baris berikut ini (nama domain) :

zone "network.athome" {

        type master;

        file "/etc/bind/db.network";

        allow-update { key "rndc-key"; };

        notify yes;

};

zone "0.168.192.in-addr.arpa" {

        type master;

        file "/etc/bind/db.192.168.0";

        allow-update { key "rndc-key"; };

        notify yes;

};

include "/etc/bind/rndc.key";

Create file rndc-key pada /etc/bind jk belum ada dan isi sbb :

key "rndc-key" {

        algorithm       hmac-md5;

        secret          "lgkbhjhtthgtlghtl6567==";

};

Edit file /etc/dhcp3/dhcp3.conf, tambahkan berikut :

# Basic stuff to name the server and switch on updating

server-identifier           server;

ddns-updates                on;

ddns-update-style           interim;

ddns-domainname             "network.athome.";

ddns-rev-domainname         "in-addr.arpa.";

ignore                      client-updates;

# This is the key so that DHCP can authenticate it's self to BIND9

include                     "/etc/bind/rndc.key";

# This is the communication zone

zone network.athome. {

    primary 127.0.0.1;

    key rndc-key;

}

zone    0.168.192.in-addr.arpa. {

            primary 192.168.0.60;

            key             "rndc-key";

    }

Selanjutnya pada /etc/dhcp3/dhclient.conf tambahkan baris berikut :

send host-name "mycomputer";
Lakukan restart dns dan dhcp

Dari client jalankan dhclient

